16 Bit Addition

**Program:**

LDA 2000

MOV B,A

LDA 2001

MOV C,A

LDA 2002

MOV D,A

LDA 2003

ADD C

STA 2005

MOV A,D

ADD B

STA 2004

HLT

**Program output:**

