8 Bit Multiplication

**Program:**

LDA 8000

MOV B,A

LDA 8001

MOV C,A

CPI 00

JZ LOOP

XRA A

LOOP1: ADD B

DCR C

JZ LOOP

JMP LOOP1

LOOP: STA 8002

HLT

**Program output:**

